SPECIFICATIONS 
New Kia Sorento SUV 
Body & Chassis 

The new Sorento offers the choice of either a manual or automatic transmission on the 2.2 litre 5- and 7-seater diesel models, and automatic transmission only on the 3.5 litre 7-seater petrol model, This 6-speed gearbox results in excellent acceleration, higher torque capacity and smooth, fuel efficient gear changes. 
Engine

2.2-litre Diesel 

Name  


‘R2.2’ 
Type


DOHC, four-cylinder in line, with E-VGT 

Capacity 

2.2-litres, 2199 cc 

Bore & Stroke 

85.4 x 96.0 mm 

Compression ratio
16.0:1 

Max power 

146.9 kW @ 3800 rpm 

Max torque / MT
421.7 Nm @ 1800-to-2500 rpm 

 / AT


436.4 Nm @ 1800-to-2500 rpm 

Valves


16 (4-per-cylinder) 

Fuel system 

CRDi, common-rail, high pressure, direct injection 

Turbo system 

Electrical Variable geometry turbocharger (E-VGT) 

Construction 

Cast iron cylinder block and aluminium head 

Emissions class 
Euro-4
3.5-litre Gasoline 

Name 


‘Lambda ll’ 

Type 


Quad-OHC, six-cylinder,with dual CVVT 

Capacity 

3.5-litres, 3470 cc 

Bore & Stroke 

92.0 x 87.0 mm 

Compression ratio
10.6:1 

Max power 

206.6 kW @ 6300 rpm 

Max torque 

335.4 Nm @ 5000 rpm 

Valves


24 (4-per-cylinder) 

Fuel system 

Multi-point injection 

Construction 

Aluminium cylinder block and head 

Emissions class 
Euro-4 

KIA SORENTO / TECHNICAL SPECIFICATIONS
Transmissions

 2.2 D


3.5 P
Manual  

 6-sp 


  ---

Automatic  

 6-sp 


6-sp
Gear Ratios 

2.2 D MT/AT


3.5P AT 
1 


3.538 / 4.212 


4.615
2


1.909 / 2.637 


2.831
3


1.179 / 1.800 


1.842
4


0.814 / 1.386 


1.386
5


0.737 / 1.000 


1.000
6


0.628 / 0.772


0.772 

Reverse

3.910 / 3.385 


3.393
Final Drive 

4.750 / 3.913 


3.195
Final Drive 
 
4.071 / ----


   --- 

Drivetrains 

4-wheel drive (part-time) 

Electronically controlled single ratio (High) system delivers 100% of torque to front wheels during normal road driving.  Manually selected ‘Lock Mode’ splits torque 50/50 between front/rear axles for enhanced stability during slippery conditions (up to 30 km/h). Safety aided by electronic Traction Control, ABS Anti-lock Braking and ESC with Downhill Brake Control and Hill-start Assist Control.

2-wheel drive 

Delivers 100% of torque to the front wheels. Safety aided by electronic Traction Control, ABS anti-lock braking and ESC with Downhill Brake Control and Hill-start Assist Control. 

Suspension & Damping 

Front 
Fully independent by subframe-mounted Macpherson struts, with coil springs and gas-filled shock absorbers. Anti-roll stabiliser bar.

Rear 
Fully independent by subframe-mounted multi-links, coil springs and gas-filled shock absorbers - with self-levelling system on 7-seater.
Steering

Type 


Hydraulic power-assisted rack and pinion 

Overall ratio 

15.35:1 

Gearing 

3.02 turns lock-to-lock 

Turning circle 

10.88 metres 

Brakes

Power 


Single 11-inch booster 

Front  
 

321 x 28 mm ventilated discs 

Rear 


302 x 11 mm solid discs 

ABS 


4-Channel anti-lock system with EBD 

BAS


Boosts braking power during emergency stops 

DBC 


Downhill Brake Control maintains 8 km/h speed during descents 
HAC


Hill-start Assist Control system to prevent rollback. 
Wheels & Tyres 
Standard: 5-Seater  
Alloy 17 in x 7.0J 
235/65 R17 tyres 

Standard: 7-Seater 
Alloy 18 in x 7.0J 
235/60 R18 tyres 

Spare 

 
Full size alloy wheel and tyre 

KIA SORENTO / TECHNICAL SPECIFICATIONS 
DIMENSIONS (mm)

Exterior

Overall length 

4685 

Overall width* 

1885 

Overall height 

1710 

Wheelbase 

2700 

Front track 

1618 

Rear track 

1621 

Front overhang
  945 

Rear overhang 
1040 

Ground clearance 
  184 

*excluding door mirrors 

Approach angle 
  25.1 degrees 

Departure angle 
  23.1 degrees 

Ramp over angle
  17.1 degrees 

Interior 

Front 

Middle

Rear 

Headroom 

1022

  995

  906 

Legroom 

1095

  955

  795 

Shoulder room 
1506

1491

1366 

Hip room

1431

1421

1128 

Capacities 

Fuel tank 

  70 litres 

Luggage (SAE) 
  258 litres
(behind 3rd row seats) 

1047 litres  
(behind 2nd row seats) 




2052 litres
(behind 1st row seats) 

Weights (kg) 

4-wheel drive

2.2D MT / AT 

3.5P AT
Curb weight (min.)
1760 / 1810 

1760
Gross weight 

2510 / 2510 

2510
2-wheel drive 

Curb weight (min.)
1720 / 1750 

  ---
Gross weight 

2510 / 2510 

  ---
Performance 

4-wheel drive

2.2D MT / AT 

3.5P AT
Top speed / kph 
190 / 190 

190
0-to-100 kph / sec 
9.6 / 10.0 

 8.1
100-to-0 kph / m
42.8


 42.8 



Towing (max) kg* 
2000 / 2000

 2000
2-wheel drive 

Top speed / kph 
190 / 190 

  ---
0-to-100 kph / sec 
9.4 / 9.7

  ---
100-to-0 kph / m
42.8 


  ---
Towing (max) kg* 
2000 / 2000 

  ---
*trailer with brakes 
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Fuel Economy (litres/100 km)* 

4-wheel drive

2.2D MT / AT 

3.5P AT (Available 2010)
Combined cycle 
6.6 / 7.4 

     ----
CO2 g/km

174 / 194 

     ----
2-wheel drive 

Combined cycle 
6.5 / 7.2 

     ----
CO2 g/km 

171 / 189

     ----

Maintenance plan is 5 Year / 100 000km

Warranty is 5 Year / 100 000km

3 Year / Unlimited km Road

Service intervals:

Petrol: Service intervals are at 15000 km / 1 year

Diesel: Service intervals are at 20000 km / 1 year

*Kia Motor Corporation test results 

